/* Do Not remove First 2 lines, Makefile will modify these lines with proper board names */
board=atmel_at91sam9x25ek
board_name=atmel,at91sam9x25ek
bootargs=console=ttyS0,115200 earlyprintk root=/dev/mmcblk0p2 rw rootwait rootfstype=ext4
bootargsd2=console=ttyS0,115200 earlyprintk root=/dev/mmcblk1p2 rw rootwait rootfstype=ext4
bootargsxx=console=ttyS0,115200 earlyprintk root=/dev/mmcblk0p2 rw rootwait rootfstype=ext4
bootcmd=run setloadaddr; run setbootargs; run fatload_mmc; bootm ${loadaddr}
bootdelay=1
fatload_mmc=if test ${board_name} = atmel,sama5d2-xplained || test ${board_name} = microchip,sama7g5ek; then fatload mmc 1:1 ${loadaddr} ${board}-fit.itb; else fatload mmc 0:1 ${loadaddr} ${board}-fit.itb; fi
setbootargs=if test ${board_name} = atmel,sama5d2-xplained || test ${board_name} = microchip,sama7g5ek; then setenv bootargs ${bootargsd2}; else setenv bootargs ${bootargsxx}; fi
setloadaddr=if test ${board_name} = microchip,sama7g5ek; then setenv loadaddr 0x63000000; else setenv loadaddr 0x21000000; fi
ethact=gmac0
stderr=serial
stdin=serial
stdout=serial
